Canlift CL-07



**CL-07  
Lift Landing Door Retering Cam**  
  
 **»** High quality and with technical features,  
  
**»** Convenient assembly and hardness,  
  
**»** Special packaging to protect against outer factors enabling easy storage,  
  
**»** 33 mm. mobility zone  
  
**»** Voltage : 48, 60, 80, 110, 190 V. DC 220 V. AC  
  
**»** Bobbin Rotation / Hour : 240  
  
**»** Weight : 5,5 kg.  
  
**»** Two year actual guarantee.

[**Technical Drawing**](http://dapsan.com/uploads/Cizim_CL07.jpg)

[](http://dapsan.com/uploads/Cizim_CL07.jpg)