8003



FEATURES

• 4 mm galvanized sheet


• Polyamide guide shoe

• Supported by rubber

• 3 types for guides 5-9-16m

• Work speed max 1.2m/sc

**Technical Drawing**

[](http://dapsan.com/uploads/ptnczm.jpg)