8001



|  |  |  |
| --- | --- | --- |
|

|  |  |
| --- | --- |
| **FEATURES** |  |

 |
|

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|

|  |  |
| --- | --- |
| • | 4 mm galvanized sheet |
| • | Polyamide guide shoe |
| • | 2 types for guides 5-9mm |

 |

 |

**Technical Drawing**

